

Power Analysis


A constant 3.7V is necessary to run the rover!!


Schematics





2.





3.